# Armour Geddon Technical Info

Armour Geddon PC requires more than 580k free memory in some configurations. If you know how to free up this memory, please do so. Otherwise, instructions for making a DOS Boot Disk can be found here.

Some users have reported problems when using the two-player modem to modem link. Unfortunately, some modems do not appear to perform rate negotiations properly when connected to modems of other brands. The best solution is to use a null-modem cable between the two machines.

For many people this will not be possible. The next best solution is to pre-configure your modem for a permanently auto-reliable connection. On SupraFaxModems, this setting can be accomplished by typing `AT&F2` then `AT&W0` from within your terminal program. This will store the &F2 (auto-reliable) configuration as the default.

For other modems, check the documentation.